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SAFETY
Confined space entry permit
A permit-required confined space entry permit with every item OSHA 1910.146(f) asks for: the space, purpose, people, hazards, isolation, atmospheric tests, rescue and sign-off.
How often: Each entry   ·   Who: Entry supervisor   ·   About 15 min   ·   22 items
	Site or area
	
	Date and time
	

	Asset or line
	
	Completed by
	


Before you use it
1. Under OSHA 29 CFR 1910.146(e), the entry supervisor signs the permit before entry begins, it is posted at the entry portal or otherwise made available to the entrants, and it lasts no longer than the job needs.
1. The entry supervisor cancels the permit when the work is done, or when a condition the permit does not allow arises. Keep cancelled permits for at least a year, with any problems noted on them.
1. This template follows the items listed in 1910.146(f). Fill in your program’s acceptable entry conditions and test order; it does not replace your written permit-space program.
Space and purpose
	NO.
	ITEM
	RESULT
	NOTES

	1
	Scan the space’s tag
	 Visited
	

	2
	Permit space to be entered
	


	3
	Purpose of the entry
	


	4
	Date and authorized duration
	



People
	NO.
	ITEM
	RESULT
	NOTES

	5
	Authorized entrants, or the roster used to track them
	


	6
	Attendants, by name
	


	7
	Entry supervisor, by name
	



Hazards and controls
	NO.
	ITEM
	RESULT
	NOTES

	8
	Hazards of the space
	


	9
	Isolation and controls: lockout, purging, inerting, ventilating, flushing
	


	10
	Acceptable entry conditions
	



Atmospheric tests
	NO.
	ITEM
	RESULT
	NOTES

	11
	Oxygen
OSHA counts below 19.5% or above 23.5% as a hazardous atmosphere.
	____________  %
Limit  ____________
	

	12
	Flammable gases and vapors
OSHA counts more than 10% of the lower flammable limit as a hazardous atmosphere.
	____________  % LEL
Limit  ____________
	

	13
	Toxic gases
Test for the substances your hazard assessment names, against their exposure limits.
	____________  ppm
Limit  ____________
	

	14
	Tester’s initials and time of each test
	


	15
	Periodic test results, with times and initials
	



Rescue, communication and equipment
	NO.
	ITEM
	RESULT
	NOTES

	16
	Rescue and emergency services, and how to summon them
	


	17
	How entrants and attendants stay in contact
	


	18
	Equipment: PPE, testing, communications, alarms, rescue
	


	19
	Other permits issued, such as hot work
	



Authorization and close-out
	NO.
	ITEM
	RESULT
	NOTES

	20
	Entry supervisor authorizing entry
	Name  ______________________________
Signature  ______________________________
Date  ______________________________

	21
	Permit cancelled because
	 Work complete     A condition the permit does not allow
	

	22
	Problems encountered during the entry
	



Follow-up
For each failed check or reading out of limit: what was found, what was done, and the work order raised for it.
	NO.
	WHAT WAS FOUND
	ACTION OR WORK ORDER
	OWNER
	DUE

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


References
1. OSHA 29 CFR 1910.146, permit-required confined spaces
Free to use and adapt. To run it on mobile, with checkpoint scans, readings checked against their limits as they are entered, and photos and signatures attached to the check, see vardian.io/templates/confined-space-entry-permit.
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