[image: ]	Free checklist template · vardian.io/templates/hot-work-permit
SAFETY
Hot work permit
The permit for welding, cutting and other hot work: the area inspected, combustibles within 35 feet removed or protected, a fire watch, and a final check after the work ends.
How often: Each job   ·   Who: Permit issuer and fire watch   ·   About 10 min   ·   14 items
	Site or area
	
	Date and time
	

	Asset or line
	
	Completed by
	


Before you use it
1. OSHA 29 CFR 1910.252(a)(2)(iv) requires the area to be inspected by the person responsible for authorizing welding and cutting, who designates the precautions, preferably in a written permit.
1. A fire watch is required where more than a minor fire might develop, for example when appreciable combustibles are closer than 35 feet, and it stays for at least half an hour after the work ends (1910.252(a)(2)(iii)).
1. Combustible material on the floor is swept clean for a 35-foot radius (1910.252(a)(2)(v)). Add your site’s and your insurer’s own hot work rules.
Job
	NO.
	ITEM
	RESULT
	NOTES

	1
	Scan the work location’s tag
	 Visited
	

	2
	Location and equipment
	


	3
	Work
	 Welding     Cutting     Grinding     Brazing or soldering
	

	4
	Permit valid from and to
	



Precautions
	NO.
	ITEM
	RESULT
	NOTES

	5
	Area inspected by the person authorizing the work
	 Pass     Fail     N/A
	

	6
	Combustibles within 35 feet removed or covered with fire-resistant shields
	 Pass     Fail     N/A
	

	7
	Floor swept clean within 35 feet; combustible floors wet or covered
	 Pass     Fail     N/A
	

	8
	Wall and floor openings within 35 feet covered
	 Pass     Fail     N/A
	

	9
	Fire extinguisher at the work location
	 Pass     Fail     N/A
	


Fire watch
	NO.
	ITEM
	RESULT
	NOTES

	10
	Fire watch assigned, with an extinguisher and trained to use it
	 Pass     Fail     N/A
	

	11
	Fire watch kept at least 30 minutes after the work ended
	 Pass     Fail     N/A
	

	12
	Time of the final check
	



Sign-off
	NO.
	ITEM
	RESULT
	NOTES

	13
	Permit issuer
	Name  ______________________________
Signature  ______________________________
Date  ______________________________

	14
	Fire watch
	Name  ______________________________
Signature  ______________________________
Date  ______________________________


Follow-up
For each failed check or reading out of limit: what was found, what was done, and the work order raised for it.
	NO.
	WHAT WAS FOUND
	ACTION OR WORK ORDER
	OWNER
	DUE

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


References
1. OSHA 29 CFR 1910.252, welding, cutting and brazing: general requirements
Free to use and adapt. To run it on mobile, with checkpoint scans, readings checked against their limits as they are entered, and photos and signatures attached to the check, see vardian.io/templates/hot-work-permit.
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