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INSPECTIONS
Overhead crane daily inspection checklist
The daily pre-use check of an overhead or gantry crane: controls, brakes, limit switch, hook, and hoist chain or rope, signed so it can serve as the monthly record too.
How often: Daily, before first use   ·   Who: Crane operator   ·   About 5 min   ·   16 items
	Site or area
	
	Date and time
	

	Asset or line
	
	Completed by
	


Before you use it
1. OSHA 29 CFR 1910.179(j) divides inspections of cranes in regular service into frequent (daily to monthly) and periodic (1 to 12 months). Operating mechanisms and air or hydraulic systems are checked daily.
1. Hooks and hoist chains get a visual check daily and a monthly inspection with a certification record: the date, the signature of the person who inspected and the hook or chain identifier. Running ropes get a thorough inspection at least monthly, with the same kind of record.
1. Use this sheet for the daily check. For the monthly record, complete the hook, chain and rope items in full, add their identifiers and keep the signed sheet on file.
Crane
	NO.
	ITEM
	RESULT
	NOTES

	1
	Scan the crane’s tag
	 Visited
	

	2
	Rated load marking legible
	 Pass     Fail     N/A
	

	3
	Area below clear; warning devices work
	 Pass     Fail     N/A
	


Controls and brakes
	NO.
	ITEM
	RESULT
	NOTES

	4
	Pendant or radio controls work and are labeled
	 Pass     Fail     N/A
	

	5
	Hoist, trolley and bridge motions respond correctly
	 Pass     Fail     N/A
	

	6
	Upper limit switch stops the hook
	 Pass     Fail     N/A
	

	7
	Brakes hold and stop smoothly
	 Pass     Fail     N/A
	

	8
	No leaks in air or hydraulic lines, tanks or valves
	 Pass     Fail     N/A
	


Hook and hoist
	NO.
	ITEM
	RESULT
	NOTES

	9
	Hook free of cracks, deformation and twist
	 Pass     Fail     N/A
	

	10
	Hook safety latch works
	 Pass     Fail     N/A
	

	11
	Chain or rope free of excess wear, kinks, twist or broken wires
	 Pass     Fail     N/A
	

	12
	Chain or rope seated correctly on the drum and sheaves
	 Pass     Fail     N/A
	

	13
	Hook and chain or rope identifiers (monthly record)
	



Result
	NO.
	ITEM
	RESULT
	NOTES

	14
	Result
	 In service     Removed from service
	

	15
	Photo of any defect
	 Photo taken
	

	16
	Inspector
	Name  ______________________________
Signature  ______________________________
Date  ______________________________


Follow-up
For each failed check or reading out of limit: what was found, what was done, and the work order raised for it.
	NO.
	WHAT WAS FOUND
	ACTION OR WORK ORDER
	OWNER
	DUE

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


References
1. OSHA 29 CFR 1910.179, overhead and gantry cranes
Free to use and adapt. To run it on mobile, with checkpoint scans, readings checked against their limits as they are entered, and photos and signatures attached to the check, see vardian.io/templates/overhead-crane-inspection-checklist.
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