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SAFETY
Walking-working surfaces and housekeeping inspection checklist
The regular inspection OSHA 1910.22(d) requires of floors, aisles, stairs, platforms and passageways: clean, dry and orderly surfaces, hazards guarded until they are repaired, loads and safe access.
How often: Weekly, and as necessary   ·   Who: Area supervisor   ·   About 15 min   ·   18 items
	Site or area
	
	Date and time
	

	Asset or line
	
	Completed by
	


Before you use it
1. OSHA 29 CFR 1910.22(d)(1) requires walking-working surfaces to be inspected “regularly and as necessary” and maintained in a safe condition. It sets no interval, so the weekly frequency here is a starting point for the site to adjust.
1. Surface conditions under 1910.22(a): all places of employment, passageways, storerooms, service rooms and walking-working surfaces kept clean, orderly and sanitary; each workroom floor clean and, to the extent feasible, dry, with drainage maintained and dry standing places such as false floors, platforms and mats provided where wet processes are used; and surfaces maintained free of hazards such as sharp or protruding objects, loose boards, corrosion, leaks, spills, snow and ice.
1. A hazardous condition must be corrected or repaired before an employee uses the surface again. If that cannot be done immediately, the hazard must be guarded to prevent employees from using the surface until it is corrected or repaired (1910.22(d)(2)). A correction or repair that involves the structural integrity of the surface must be performed or supervised by a qualified person (1910.22(d)(3)).
1. Each walking-working surface must support its maximum intended load (1910.22(b)), and the employer must provide, and ensure each employee uses, a safe means of access to and from walking-working surfaces (1910.22(c)). Add the site’s own items for guardrails, floor holes and dock edges, which other sections of subpart D cover.
1. Run the checklist per area or building section, and attach a photo to every hazard so the work order shows the exact spot.
Area
	NO.
	ITEM
	RESULT
	NOTES

	1
	Scan the area tag
	 Visited
	

	2
	Area or building section
	


	3
	Surface type
	 Floor and aisles     Stairs and ramps     Platform or mezzanine     Dock or loading area     Outdoor walkway
	


Surface condition (1910.22(a))
	NO.
	ITEM
	RESULT
	NOTES

	4
	Floors, passageways and storerooms clean, orderly and free of debris
	 Pass     Fail     N/A
	

	5
	Floor dry; spills and leaks cleaned up, and drainage working where wet processes run
	 Pass     Fail     N/A
	

	6
	Dry standing places such as mats, false floors or platforms in place at wet processes
	 Pass     Fail     N/A
	

	7
	No sharp or protruding objects, loose boards or corrosion
	 Pass     Fail     N/A
	

	8
	No snow or ice on walkways and outdoor surfaces
	 Pass     Fail     N/A
	

	9
	Aisles and passageways clear for their full width
	 Pass     Fail     N/A
	


Loads and access (1910.22(b)–(c))
	NO.
	ITEM
	RESULT
	NOTES

	10
	Stored materials within the rated load of the floor, platform or mezzanine
	 Pass     Fail     N/A
	

	11
	Safe means of access and egress to each platform, mezzanine and elevated surface in place and in use
	 Pass     Fail     N/A
	

	12
	Stairs, ramps and ladders used for access in sound condition
	 Pass     Fail     N/A
	


Hazards found (1910.22(d))
	NO.
	ITEM
	RESULT
	NOTES

	13
	Each hazard corrected before the surface is used again, or guarded off until it is
	 Pass     Fail     N/A
	

	14
	Repairs affecting structural integrity assigned to, or supervised by, a qualified person
	 Pass     Fail     N/A
	

	15
	Photo of each hazard
	 Photo taken
	

	16
	Location and description of each hazard
	



Result
	NO.
	ITEM
	RESULT
	NOTES

	17
	Result
	 No hazards     Hazards guarded, work orders raised     Area closed until repaired
	

	18
	Inspector
	Name  ______________________________
Signature  ______________________________
Date  ______________________________


Follow-up
For each failed check or reading out of limit: what was found, what was done, and the work order raised for it.
	NO.
	WHAT WAS FOUND
	ACTION OR WORK ORDER
	OWNER
	DUE

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	


References
1. OSHA 29 CFR 1910.22, walking-working surfaces: general requirements
Free to use and adapt. To run it on mobile, with checkpoint scans, readings checked against their limits as they are entered, and photos and signatures attached to the check, see vardian.io/templates/walking-working-surfaces-inspection.
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